PRE/MAIN section
Power output : 	2x 40W (continuous, 20Hz...20Khz, 8 Ohm, 0,05% THD)
IMD : 	no more than 0,05% (8 Ohm, both channels driven)
Frequency response : 	10Hz...50Khz (-1dB)
Input sensitivity : 	2,5mV (phono)
150mV (aux, monitor)
Phono overload voltage :  150mV (1Khz)
S/N ratio : 	70dB (phono)
90dB (aux, monitor)
Residual noise : 	no more than 0,7mV
Damping factor : 	no less than 60 (8 Ohm)
Tone controls : 	±10dB at 100Hz
±10dB at 10Khz
Filters : 		70Hz (6dB/oct.)
7Khz (6dB/oct.)
Crosstalk at 1Khz : 	-65dB (aux, monitor)
FM section
Usable sensitivity : 	11,2dBf (2µV, mono)
19dBf (4,8µV, stereo)
46dB quieting : 	18,2dBf (4,5µV, mono)
41dBf (60µV, stereo)
50dB quieting : 	70 µV min.
S/N ratio : 	74dB (mono, 65dBf)
70dB (stereo, 65dBf)
Frequency response : 	30Hz...15Khz (+0,5/-1,5dB)

THD (100Hz) : 	0,2% (mono)
0,3% (stereo)
THD (1Khz) : 	0,2% (mono)
0,3% (stereo)
THD (6Khz) : 	0,3% (mono)
0,5% (stereo)
IM : 	0,2% (mono)
0,3% (stereo)
Capture ratio : 	1,2dB at 65dBf
Alternate channel selectivity : 	70dB
Spurious response ratio : 	90dB
Image response ratio : 	80dB
IF response ratio : 	85dB
AM suppression ratio : 	50dB
Stereo separation : 	45dB (100Hz)
45dB (1Khz)
40dB (10Khz)
Subcarrier product ratio : 	60dB
SCA rejection ratio : 	60dB
General
PC : 	170W at rated power
Dimensions : 	48.5 x 35.3 x 17.5cm
Weight : 	12kg.